Full Maintenance Schedule
Weekly
☐ Wipe X & Y rails clean. or blow off with air ensure 
there is no foam around belts 
☐ Inspect X/Y belts for wear.
☐ Check trolley alignment.
☐ Clean wire guides.
Monthly
☐ Inspect axis ball bearings.
☐ Lubricate linear bearings (OF/OC).
☐ Test E-Stop cable .
☐ Inspect tension spring.
☐ Inspect belt tension both sides to be equal 
☐ Check cooling fans.
General / As Needed
☐ Clean proximity switches.
☐ Replace worn wires.
☐ Keep machine clean.
Environment Requirements
• Temperature: 5–35°C.
• Humidity: 30–75% non-condensing.
• Proper grounding required.
Weekly Sign-Off
Technician Name: ____________________________
Date: ____________________________
Supervisor Signature: ____________________________
