/Preventive Maintenance Schedule —  Overhead Crane
Monthly PM (Qualified Technician)
• Hook inspection (deformation, cracks, latch condition)
• Wire rope/chain condition (broken strands, wear, kinks, corrosion)
• Sheave rotation and wear
• Hoist drum rope spooling
• Limit switch verification
• Pendant/radio control function
• Festoon/cable track condition
• Trolley/bridge travel check
Technician Name: ______________________________
Technician Signature: __________________________
Date: ____________________

Quarterly PM (Qualified Technician)
• All monthly PM items
• Brake inspection and functional test
• Motor brush inspection
• Gearbox oil level check and leak inspection
• Wheel and bearing wear
• Couplings, shafts, and keys inspection
• Runway and bridge alignment visual check
• Overload protection device test
Technician Name: ______________________________
Technician Signature: __________________________
Date: ____________________

Semiannual PM (Qualified Technician)
• All monthly + quarterly items
• Full structural component check
• Electrical panel cleaning and terminal inspection
• End stops and bumper inspection
• Runway bolts/clips inspection
• Bearing and sheave lubrication
• Drive system gear wear check
• Motor and gearbox performance evaluation
Technician Name: ______________________________
Technician Signature: __________________________
Date: ____________________

Annual PM (Qualified Technician)
• All lower-level PM items
• Annual load test per OSHA/ASME requirements
• Structural inspection
• Hook and load-bearing NDT (if required)
• Complete electrical system inspection
• Review and update of maintenance schedule
Technician Name: ______________________________
Technician Signature: __________________________
Date: ____________________





Daily Crane Operator Visual Inspection Checklist — 15-Ton Overhead Crane
Date: ____________________
Operator: ____________________
Crane ID/Location: ____________________

Hook & Load Block
☐ Hook not bent or twisted
☐ No cracks or gouges
☐ Safety latch working
☐ Hook rotates freely
Wire Rope / Chain
☐ No broken strands or links
☐ No kinks, birdcaging, or crushed areas
☐ Proper seating in drum/sheaves
☐ No corrosion or excessive wear
Hoist Operation
☐ Smooth lifting and lowering
☐ No abnormal noise
☐ No load slipping or drifting
☐ Limits working during normal use
Trolley & Bridge
☐ Smooth travel (no binding)
☐ No abnormal vibration or noise
☐ Bumpers in place
Controls
☐ Pendant/remote functions correctly
☐ Emergency stop working
☐ No visible wire damage

Electrical / Mechanical
☐ No visible leaks
☐ Festoon/cable track moves properly
☐ No burning smell or hot spots
Environment / Safety
☐ Area below crane is clear
☐ Warning labels visible
☐ Load within rated capacity
Issues Found (Operator Notes)




Technician Resolution Sign-Off
Technician Name: ______________________________
Corrective Action Taken:




Technician Signature: __________________________
Date: ____________________
